NOTES:
21	Torque to 50-60 in.-lb.
48	Torque to 30-40 in.-lb.
65		Torque to 25-30 in-lb.
93	Torque to 25-30 in.-lb. Bend tabs on washer to trap nut.
97, 122	Torque to 7-10 in.-lb.  Use Loctite 290.
103	Lip on seal next to bearing faces bearing, seal next to sprocket faces sprocket.
Change Oil Every 50 Operating Hours

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.