NOTES:
1	Date Code:  located on side of handle
21	Nut to be finger tight prior to applying final tightening torque of 80-90 in.-lb.
39	Lubricate with motorcycle chain lube
48	Torque to 30-40 in.-lb.
65	Torque to 25-30 in.-lb.
90	Assemble tightly into angled grove in Seal sleeve (item 89) prior to assembly against inner race of ball bearing (item 99).
93	Torque to 60-65 in.-lb.
97	122 Torque to 7-10 in.-lb.  Use Loctite 290.
98	Coat wiping edge (lip) of Seal with Band Saw Gear Lube prior to installing Seal Sleeve (item 89)
99	Inner race of Ball Bearing that faces Seal to be free of grease and oil.
103	Lip on seal next to bearing faces bearing, seal next to sprocket faces sprocket
125	Orient such that blade rides across chamfers. 

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.