NOTES:
	7-		Seal to face commutator.
	18-		Date Code: Located on inside of cover half (see diagram).

LUBRICATION:
Distribute 21 grams of  Polyrex grease in gear case.

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.