NOTES:
	9-		Press bearing flush with end of shaft; shield to face commutator.
	10,33-		Press to bottom of bore; seal to face gear.
	12,51	Units with long brush leads do not have these terminals.
	17-		Date code: bottom of field case.
	29-	Coat clutch face with B&D clutch grease.
	37-		Bearing to be pressed to shoulder.
	43-		Some bit holders built with O-Ring & Cap assembly.
	50-		Assemble seal with lip facing away from threads.
	58-	Torque to 6.8-8.0 n.m (60-70 in.-lbs).
	60-		Assemble seal with lip toward gear case. Press to bottom of bore in bearing.

LUBRICATION:
Distribute 9/16 oz. of grease in gear case.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.