NOTES:
	3-	Date Code: located on bottom of housing cover.
	7-	Seal to face threads.
	30-	Concave side to face item 11 (gear).
	31-	For units prior to date code 901.

LUBRICATION:
Fill gear case with 1/8 oz. of grease.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.