NOTES:
	3-		Date Code:Located inside of cover half (see diagram).
	7-		Front edge of clutch should be pressed to 1.15" from shoulder of spindle.
	7-		Clutch adjustment:  While looking at front of unit, assemble adjusting nut (item 18) clockwise until flush
with threads on housings. Align clutch teeth so the tops of the teeth touch each other. Loosen adjusting nut counterclockwise until front face is 3/16" from front of output spindle. Assemble adjusting collar over adjusting nut with no. "1" on the Collar aligned with the indicator on the Housings.
	37-		Some units built with this part.

LUBRICATION:
Distribute 3/8 oz. of Polyrex grease in gear case.

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.