LUBRICATION:
Distribute 20 grams (5/8 oz.) of Lidok EP-1 grease into gear case. Coat gear teeth.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.