NOTES:
	2,6	Torque to 20-25 ft./lbs.

	3	Assemble bearing with circumferential groove or etched race faced toward gear.

	4,15	Add grease to inside splines before assembly.

	5	Concave sides down towards gear.

	10	Torque to 150-170 in./lbs.

	14	Torque to 50-70 in./lbs., then loosen 1/8 turn.

	24	Assemble with seal side toward commutator.

	39,40	A: If brush cover is shaped like:

		order: Brush Cover 39A (1) and  Screw 40A (2)

		B: If brush cover is shaped like:

		order: Brush Cover 39B (1) and Screw 40B (2)

	55	Position 1st washer with concave side toward bearing. Position 2nd washer with concave side toward locking ring.

LUBRICATION:
Distribute 6 oz. of grease in gear case. Coat gear teeth.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.