NOTES:
1 Torque 30-35 in. lbs.
6,51 Blade assembly screws to be tight, loosen up to ¾ turn if necessary
16 When using shaft 464226-00 press flush to top of gear case
21 Assemble with concave side toward fan
32,33 Torque 12-14 in. lbs.
36 Date Code located on cover side of field case.
50 Torque 12-18 in/ lbs.

LUBRICATION:
Apply small amount of ML 54
Grease in area
Of parts 8,9,12,14
Fill gear case (17) with 5/8-7/8 oz.
Of ML 54 grease

CAUTION:
When servicing Double Insulated Tools, it is extremely important that ONLY IDENTICAL REPLACEMENT PARTS BE USED and that REASSEMBLY OF TOOL IS IDENTICAL TO THE ORIGINAL ASSEMBLY.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.