NOTES:
	9-		Press flush with end of shaft; seal to face commutator.
	10-		End of shaft to bearing; 1.048-1.052"; seal to face fan.
	13-		Assemble bearing to depth of 1.024- 1.043" below mounting surface to gear case.
	23-		Date Code: bottom of field case.

LUBRICATION:
Distribute 3.0 oz. (85 grams) of BD-L2.0 grease in gear case.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.