Black & Decker Corp.                                                           
                   USA SERVICE OPERATIONS
 	TECHNICAL SERVICES DEPARTMENT			SB06106

                 		SERVICE BULLETIN					PAGE 1 OF 1

                          									ISSUED: December 10, 2008
											Revised: March 8, 2012
											Written By: K. Butler
SUBJECT:  SAFETY TEST PROCEDURE
UNITS:  D55146, D55146-CA, D55167, D55168, D55168-CA, SEARS 919-16760, 919-16761, 919-16762, 919-16763, 919-16770 & 919-16771, CAP1615-OF, CAP1645-OF
DATE CODES AFFECTED:  ALL

Before safety testing the above units, it will be necessary to remove the shroud and use compressed air to blow the brush residue from the brush holder area.  Be sure to wear eye protection.  The unit will likely fail the hipot test if this is not done because the brush has a fairly high oil content.  The unit should then be tested at no more than 1250 volts AC.