NOTES:
5	Date Code located on bottom.	
25	Torque to 9 – 11 Nm (80 – 97 In-Lbs.) {6.5 – 8.0 Ft-Lbs.}	
35, 41	Torque to 1.4 – 1.6 Nm (12.5 – 14.0 In-Lbs.)	
38	Torque to 0.45 – 0. 65 Nm (3.91 – 7.75 In-Lbs.)	
44	Torque to 2.0 – 3.0 Nm (17.7 – 16.6 In-Lbs.)	
50	Torque to 2.2 – 2.4 Nm (19.5 – 21.3 In-Lbs.)	

LUBRICATION:
10, 25		Distribute 10 - 12 grams of grease over teeth.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.