Title: NOTES:
Author: Rose Bean
Last saved by: Bixler, Clark
Company: Black & Decker

NOTES:
  1		Date Code located in battery recess.
  6		Torque to 1.2 – 1.4 Nm (10.6 – 12.4 in-lbs).
  8		Torque to 1.4 – 1.6 Nm (12.4 – 14.2 in-lbs).
25		Torque	to 2.6 – 3.0 Nm (23.0 – 26.6 in-lbs).
32		Torque	to 0.7 – 0.9 Nm (6.2 –8.0 in-lbs).

LUBRICATION:
   3			Apply 0.025 grams grease to terminals.
800		For Transmission lubrication refer to the Grease Placement Document.

CAUTION:
When servicing Double Insulated Tools, it is extremely important that ONLY IDENTICAL REPLACEMENT PARTS BE USED and that REASSEMBLY OF TOOL IS IDENTICAL TO THE ORIGINAL ASSEMBLY.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.