f NOTES:
	315 Date code located on bottom of handle and cover assy.

	318 Cord clamp to be installed with flat side against cable.

   319 Torque to 13-18 inch lbs.

   321 Torque to 8-12 inch lbs.

   323 torque to 15-22 inch lbs.

    327,328 Torque to 20-25 inch lbs.   

CAUTION:
When servicing Double Insulated Tools, it is extremely important that ONLY IDENTICAL REPLACEMENT PARTS BE USED and that REASSEMBLY OF TOOL IS IDENTICAL TO THE ORIGINAL ASSEMBLY.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.