DEWALT Hydraulic Tools - Physical Inspection Table

(Applies to DCE200, DCE300, DCE350)

|  |  |  |  |
| --- | --- | --- | --- |
| Inspection Item Number | Item to Inspect | Inspect for | Corrective Action |
| 1 | Housing | Cracking, galling, discoloration, or other damage | Replace Housings  |
| 2 | Labels | Make sure all labels are present and undamaged with serial number legible | Replace Labels and etch proper serial number is on label |
| 3 | Loose or missing screws | Loose or missing screws | Replace and tighten screws |
| 4 | Battery Terminal | Battery slides in and out properly and latches into place | Replace housings or electronics module as necessary |
| 5 | Electronics Cover | Cracking or damage to label | Replace electronics cover and/or label as necessary |
| 6 | Head | Cracks or warping | Replace head |
| 7 | USB Rubber Cover | Confirm cover is present and functional | Replace cover |
| 8 | Leaking | Leaking of the hydraulic body | Replace and repair parts as required to stop leak, reference service manual for troubleshooting steps |
| 9 | Release Trigger | When the tool has been partially actuated make sure the piston returns when the top trigger is pulled | Reference service manual |
| 10 | Motor Trigger | Starts motor and no physical damage | Replace trigger or electronics as necessary |
| 11 | Battery Foot LED | Ensure the LED lights up when the trigger is pulled and lens is present | Replace electronics module or lens as necessary |
| 12 | Latch on Head(DCE200) | Missing pieces and proper operation when jaws are inserted | Replace latch system parts |
| 13 | Jaws fit(DCE200) | Jaws slide freely in and out of tool | Replace head as necessary |
| 14 | Guide Rail(DCE300) | Make sure the guide rail on the neck is not cracked | Replace guide rail as necessary |
| 15 | Dies fit(DCE300) | Dies slide freely in and out of tool | Replace head or die holder as necessary |