NOTES:
1	Date Code located in Battery Foot area.	
9	Torque to 1.5 – 1.7 Nm (13.2 – 15.0 in. lbs.).	
11,35	Torque to 3.8 – 4.2 Nm (33.6 – 37.2 in. lbs.).	
17	Torque to 25.0 – 29.0 Nm (18.4 – 21.4 in. ft.). Left Hand Thread	
26, 40	Torque to 4.1 – 4.5 Nm (36.3 – 39.8 in. lbs.).	
32	Torque to 2.8 – 3.2 Nm (24.8 – 28.3 in. lbs.).	

LUBRICATION:
5
800	Apply 0.025 grams grease to terminals.
Grease TBD

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.