NOTES:
1	Date Code located on bottom of handle.	
14	Torque to 1.2 to 1.5 Nm (11 to 13 in. lbs).	
30	Torque to 1.5 to 1.8 Nm (13 to 16 in. lbs).	
34	Torque to 1.7 to 1.9 Nm (15 to 17 in. lbs).	
35
36, 37
40	Torque to 3.3 to 3.8 Nm (29 to 34 in. lbs).
Torque to 3.5 to 4.0 Nm (31 to 35 in. lbs).
Torque to 4.5 to 5.0 Nm (40 to 44 in. lbs).	
106	Torque to 3.0 to 3.5 Nm (27 to 31 in. lbs).	

LUBRICATION:
Apply 8 – 10 grams of grease on the Gear and Pinion.

CAUTION:
Static electricity can damage electronic components. Repair only at static-free station. Refer to SDB 5955.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.