Function Checks 
 
•	 Bypass Function Check - Saw shall not actuate without Blade Guard Assembly, light should blink constantly 
•	Test the bypass switch - Make sure light blinks, then bypass, make sure light goes solid – saw turns on 
•	Pull up on Guard Assembly, Light shall not turn on or blink. 
•	Test No Volt function – turn on, cut power, turn power back on – saw must not run.