NOTES:
1		Date code located on right side of housing above identification label.  Also order items 34 and 35. 
11	Cord jacket must extend beyond clamp by at least 2.0mm (3/32”).
13	Torque cord clamp screws to 10-14 in-lbs.
25	Convex side toward pad.
60	Bearing inner race to be flush to 0.2mm (.008”) below end of armature shaft.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.