NOTES:
When servicing item 18, 29 or 30, you must replace insulating tape (item 57) to maintain double insulating qualities of the unit. Any removal or damage to the tape requires it to be replaced. Install as shown below.

IMPORTANT!
To assure product safety and reliability, all repairs, maintenance, and adjustments should be performed by company-owned or authorized service organizations using identical replacement parts. Instructions for safe operation are included in the instruction manual that was supplied with the product.